AtsFreq / AtsAmp Use Freq and Amp data from a given partial

AtsParInfo One UGen to return both Amp and Freq info

AtsFreq.kr(atsbuffer partialNum, filePointer, mul, add);

- returns frequency information for a given partial

partialNumber - the number of the partial to return frequency data for. Partial 0 is the first partial.

AtsAmp.kr(atsbuffer, partialNum, filePointer, mul, add);

- returns amplitude information for a given partial

partialNumber - the number of the partial to return frequency data for. Partial 0 is the first partial.

AtsParInfo.kr(atsbuffer, partialNum, filePointer, mul, add);

- returns amplitude and freq information for a given partial

partialNumber - the number of the partial to return frequency data for. Partial 0 is the first partial.

Usage

For resynthesis purposes, an ATS file needs to be loaded into a buffer. When loading an ATS file, you need to supply a buffer number to store ATS data in.

s.boot;

a = AtsFile.new("sounds/a11wlk01.ats").load;

( //use freq and amp information for a filter ugen (just the first 30 partials)

{

var noise, freqs, amps, partials;

partials = Array.series(30, 1, 1);

// outputs an array of 30 freq values;

freqs = AtsFreq.kr(a.bufnum, partials, MouseX.kr(0, 1));

// outputs an array of 30 amp values

amps = AtsAmp.kr(a.bufnum, partials, MouseX.kr(0, 1));

// feed these into a reson filter, mix down to one channel

Mix.ar(Resonz.ar(WhiteNoise.ar(20), freqs, 0.01, amps));

}.play(s);

);

( //use freq and amp information for a filter ugen (just the first 30 partials)

{

var noise, freqs, amps, freqs1, amps1, partials, out;

partials = Array.series(30, 1, 1);

// outputs an array of 30 freq values;

out = AtsParInfo.kr(a.bufnum, partials, MouseX.kr(0, 1));

// need to flop the array output

#amps, freqs = out.flop;

// outputs an array of 30 amp values

// feed these into a reson filter, mix down to one channel

Mix.ar(Resonz.ar(WhiteNoise.ar(20), freqs, 0.01, amps ));

}.play(s);

);